(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(footprint "Connector_RJ:RJ45_Hanrun_HR911105A_Horizontal"
		(layer "F.Cu")
		(uuid "044bae67-fc6f-4fda-ab7b-bcaa72c7d7b0")
		(at 105.185 33.565)
		(descr "1 Port RJ45 8P8C receptacle, shielded, with magnetics, through hole, 2 LEDs, tab down, http://www.hanrun.com/public/upload/down/2020/09-11/cc11be56d66bb63d5f1eeb85492439c0.pdf")
		(tags "RJ45 Magjack ethernet")
		(property "Reference" "J4"
			(at 4.44 -5 0)
			(layer "F.SilkS")
			(uuid "546601c6-cd63-4b4d-9a3a-d59fede473cb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RJ45_Hanrun_HR911105A_Horizontal"
			(at 4.44 18.5 0)
			(layer "F.Fab")
			(uuid "9db6fe59-fb46-4017-baa6-47320580cb01")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141815_HANRUN-Zhongshan-HanRun-Elec-HR911105A_C12074.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "88441763-7904-46a2-bba5-620ae242b87d")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "21a946dc-d9f5-4b1b-a46a-5cd9acd18d68")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "RJ45*Hanrun*HR911105A*")
		(path "/ac21f246-f943-4d37-abe2-07e492592f99")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "4" "2" "3" "5" "6" "8" "SH" "7" "12" "11" "9" "10")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -3.92 -0.9)
			(end -3.92 0.9)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "fea75ec7-4e0f-42c4-9d7f-f04d7014ae75")
		)
		(fp_line
			(start -3.69 -4.15)
			(end -3.69 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "986ebc51-b6c1-4b81-9a41-60b0ccd8b6f7")
		)
		(fp_line
			(start -3.69 -4.15)
			(end 12.57 -4.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5bc2ecc3-cafb-4ebd-bdea-d208b889e65e")
		)
		(fp_line
			(start -3.69 4.93)
			(end -3.69 11.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "52876b9e-2c26-41da-815b-5061d2fb8c87")
		)
		(fp_line
			(start 12.57 -4.15)
			(end 12.57 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "47681c46-00a6-4c7d-a983-7f751c6e25b6")
		)
		(fp_line
			(start 12.57 4.93)
			(end 12.57 11.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bc815fe9-a17b-4f30-a0f8-fadb7a5b87ea")
		)
		(fp_line
			(start -5.06 2.57)
			(end -5.06 4.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "33bd93d6-88e8-453f-a31d-7a8b4de8d908")
		)
		(fp_line
			(start -5.06 2.57)
			(end -4.08 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d829148d-5ae1-4cac-9dd8-5eeef275478c")
		)
		(fp_line
			(start -5.06 4.05)
			(end -4.08 5.03)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ae5111cf-a9b0-438d-aed3-b9bbe5e58a68")
		)
		(fp_line
			(start -4.08 -4.54)
			(end -4.08 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "1e807a1e-b18a-4911-8e27-b8fa8aa9451d")
		)
		(fp_line
			(start -4.08 -4.54)
			(end 12.96 -4.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "510df9a2-d09c-490a-b0c8-afddda1c8f73")
		)
		(fp_line
			(start -4.08 5.03)
			(end -4.08 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d4870658-3790-4fc6-83b8-8240008b1b9b")
		)
		(fp_line
			(start -4.08 17.76)
			(end 12.96 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "70d73731-34aa-43a4-b3bd-9152a5479bac")
		)
		(fp_line
			(start 12.96 -4.54)
			(end 12.96 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "8fe7c19b-26df-4178-a9a6-0fab6127d313")
		)
		(fp_line
			(start 12.96 5.03)
			(end 12.96 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "20634e64-d581-49ac-8f75-5da20aa1e136")
		)
		(fp_line
			(start 13.94 2.57)
			(end 12.96 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "52406c5c-cca6-45df-a459-4983464c155b")
		)
		(fp_line
			(start 13.94 4.05)
			(end 12.96 5.03)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0ebef634-1f9f-462d-8c8d-3bb78f85504c")
		)
		(fp_line
			(start 13.94 4.05)
			(end 13.94 2.57)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "6e9253ae-8285-4b83-84df-44dea0f3e71f")
		)
		(fp_line
			(start -3.58 -4.04)
			(end -3.58 -1.01)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "d5a69861-7554-4175-9a47-1d5b3a71ffe3")
		)
		(fp_line
			(start -3.58 -4.04)
			(end 12.46 -4.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "77f36c4e-235c-412a-8b3b-5e9e479e3b32")
		)
		(fp_line
			(start -3.58 0.99)
			(end -3.58 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "342c5a7b-ba35-436a-9ffc-d308b0eae6ef")
		)
		(fp_line
			(start -3.58 17.26)
			(end 12.46 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8e218e48-fb80-4669-b279-8bd520a77659")
		)
		(fp_line
			(start -2.58 -0.01)
			(end -3.58 -1.01)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a46dd572-54e2-46b9-89c7-2b3dd20e0160")
		)
		(fp_line
			(start -2.58 -0.01)
			(end -3.58 0.99)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a852e22a-b220-4e95-b1f4-2313ca7cbc4a")
		)
		(fp_line
			(start 12.46 -4.04)
			(end 12.46 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "b423067e-e971-4e90-87cb-48ea5577b6e1")
		)
		(fp_text user "${REFERENCE}"
			(at 4.44 6.36 0)
			(layer "F.Fab")
			(uuid "f0a42312-38ee-448d-9a76-e9c645d14a76")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -1.275 6.36)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(uuid "bcb9b4d5-f005-4b0d-8547-c243d141c04b")
		)
		(pad "" np_thru_hole circle
			(at 10.155 6.36)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(uuid "edb26216-4657-4778-b218-310af587b29a")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.167)
			(net "MDI_TP_P2")
			(pinfunction "TD+_1")
			(pintype "passive")
			(uuid "c6f1df16-3cdc-4b0c-a1f7-babc7cf3446d")
		)
		(pad "2" thru_hole circle
			(at 1.26 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_TN_P2")
			(pinfunction "TD-_2")
			(pintype "passive")
			(uuid "b8291c19-1888-4d26-b4bb-50e2d5c33bd7")
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_RP_P2")
			(pinfunction "RD+_3")
			(pintype "passive")
			(uuid "baca7885-8e73-41ca-bba2-689afa4199f3")
		)
		(pad "4" thru_hole circle
			(at 3.8 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J4-TCT)")
			(pinfunction "TCT_4")
			(pintype "passive")
			(uuid "b74479ef-80bc-4a8f-a449-c080ef069940")
		)
		(pad "5" thru_hole circle
			(at 5.08 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J4-RCT)")
			(pinfunction "RCT_5")
			(pintype "passive")
			(uuid "725ed211-03ef-47ea-8a0c-4ccc2ad7d646")
		)
		(pad "6" thru_hole circle
			(at 6.34 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_RN_P2")
			(pinfunction "RD-_6")
			(pintype "passive")
			(uuid "b88381fe-bd29-4361-87a2-adb26a08c9b7")
		)
		(pad "7" thru_hole circle
			(at 7.62 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J4-NC-Pad7)")
			(pinfunction "NC_7")
			(pintype "no_connect")
			(uuid "5fdbff15-5f75-4943-9712-ae4dad7bf74d")
		)
		(pad "8" thru_hole circle
			(at 8.88 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "power_in")
			(uuid "9d290a57-ffc5-4777-8c93-b9e4f6651bc8")
		)
		(pad "9" thru_hole circle
			(at -2.185 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J4-Pad9)")
			(pintype "passive")
			(uuid "3e13849c-b7d1-4a40-9a08-e63d19342d82")
		)
		(pad "10" thru_hole circle
			(at 0.355 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J4-Pad10)")
			(pintype "passive")
			(uuid "ed6ed05b-287c-42b4-ab2b-d8a405e80f6a")
		)
		(pad "11" thru_hole circle
			(at 8.525 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J4-Pad11)")
			(pintype "passive")
			(uuid "95d7e4bc-6355-4607-880c-f2a5cc35830f")
		)
		(pad "12" thru_hole circle
			(at 11.065 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J4-Pad12)")
			(pintype "passive")
			(uuid "e58322ca-3d67-498c-a27b-9676032cd731")
		)
		(pad "SH" thru_hole circle
			(at -3.305 3.31)
			(size 2.5 2.5)
			(drill 1.63)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
			(uuid "82ddcb3d-8e1b-4122-8a89-d7d2b622278c")
		)
		(pad "SH" thru_hole circle
			(at 12.185 3.31)
			(size 2.5 2.5)
			(drill 1.63)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
			(uuid "b572f687-dbce-494f-967f-deeb0ac5e555")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Hanrun_HR911105A_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(uuid "0d41d729-15c6-4fdd-a96b-9f434108d2a5")
		(at 108.175 63.695)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(uuid "73e400dd-e146-484a-a8f6-a883d95e1646")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1k"
			(at 0 1.17 0)
			(layer "F.Fab")
			(uuid "cbaacef0-4ca1-4f3b-b1a5-cc1b971df93a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e685cd8f-faef-47f2-ac1f-c948da43ec3b")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "48b13d74-b758-474a-8349-ffeb41625548")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "802d4779-1f60-441d-9c48-10621f423f31")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7767982f-85e9-43e6-827c-11c432d57b1e")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.153641 -0.38)
			(end 0.153641 -0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "e794aff5-f546-465f-b2f3-7c2ca3c16495")
		)
		(fp_line
			(start -0.153641 0.38)
			(end 0.153641 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68791234-a451-42c2-ab95-e15307008e43")
		)
		(fp_rect
			(start -0.93 -0.47)
			(end 0.93 0.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "0fdf378e-2f38-4b98-8383-487d8e031cd7")
		)
		(fp_rect
			(start -0.525 -0.27)
			(end 0.525 0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "cc502c8c-6d0b-4f9f-aa00-c17681001599")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f44703d1-5e45-4cc1-ada6-7df69089cf31")
			(effects
				(font
					(size 0.26 0.26)
					(thickness 0.04)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J1-CC1)")
			(pintype "passive")
			(uuid "b80ce836-6093-468c-b447-311ece83f4ec")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "b3d2dc46-e6c5-421c-aaf5-554a44afdf3e")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "2171790001:MOLEX_2171790001"
		(layer "F.Cu")
		(uuid "1c7a632f-25b3-4ea2-af5d-b4542661711a")
		(at 112.345 56.655)
		(property "Reference" "J1"
			(at 0.255 -5.185 0)
			(layer "F.SilkS")
			(uuid "c4e7117a-d354-49e2-9733-e0e6a55294a4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "217179-0001"
			(at 7.24 -6.645 0)
			(layer "F.Fab")
			(uuid "353ac386-e40d-4ceb-8486-38cd2c5bb214")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "217179-0001"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "539e8957-674f-424d-ab76-578c6ab78adb")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "217179-0001"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "96811729-2c61-45c4-97e6-e366211be3bc")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(path "/000a203b-3079-4398-86da-5dce78f4e5e1")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "S_4_H2" "S_4_H1" "S_3_H2" "S_3_H1" "S_2_H2" "S_2_H1" "S_1_H2"
					"S_1_H1" "B1/A12" "1" "A1/B12" "16" "15" "14" "13" "4" "3" "B4/A9" "A4/B9"
					"A5" "B5" "A7" "B7" "A6" "B6" "A8" "B8"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_poly
			(pts
				(xy -3.5585 -4.0635) (xy -2.8415 -4.0635) (xy -2.8415 -2.7865) (xy -3.5585 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "260de215-408a-4386-bc9f-7884ee88cc39")
		)
		(fp_poly
			(pts
				(xy -2.7585 -4.0635) (xy -2.0415 -4.0635) (xy -2.0415 -2.7865) (xy -2.7585 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "9fba7a65-efd6-4484-a75f-8978b0b0ba9b")
		)
		(fp_poly
			(pts
				(xy -1.9625 -4.0635) (xy -1.5375 -4.0635) (xy -1.5375 -2.7865) (xy -1.9625 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "a48e5bb2-d8b6-4493-8588-0a6071d8c3e4")
		)
		(fp_poly
			(pts
				(xy -1.4625 -4.0635) (xy -1.0375 -4.0635) (xy -1.0375 -2.7865) (xy -1.4625 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "f673c96d-22a8-45b7-80fc-9323aa4e688e")
		)
		(fp_poly
			(pts
				(xy -0.9625 -4.0635) (xy -0.5375 -4.0635) (xy -0.5375 -2.7865) (xy -0.9625 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "8000c291-48ee-4ac0-870b-a2197f89a769")
		)
		(fp_poly
			(pts
				(xy -0.4625 -4.0635) (xy -0.0375 -4.0635) (xy -0.0375 -2.7865) (xy -0.4625 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "c301adfe-6429-45d2-ad20-c834c96d7a68")
		)
		(fp_poly
			(pts
				(xy 0.0375 -4.0635) (xy 0.4625 -4.0635) (xy 0.4625 -2.7865) (xy 0.0375 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "d7abc451-5023-45b6-9e6b-d13a3250bd36")
		)
		(fp_poly
			(pts
				(xy 0.5375 -4.0635) (xy 0.9625 -4.0635) (xy 0.9625 -2.7865) (xy 0.5375 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "d5b59a1c-83b2-4cc0-a0cf-822a582a2d70")
		)
		(fp_poly
			(pts
				(xy 1.0375 -4.0635) (xy 1.4625 -4.0635) (xy 1.4625 -2.7865) (xy 1.0375 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "fc4e63c3-4898-47a1-a495-3b5e9f79cf85")
		)
		(fp_poly
			(pts
				(xy 1.5375 -4.0635) (xy 1.9625 -4.0635) (xy 1.9625 -2.7865) (xy 1.5375 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "6fd5f615-d470-4897-a44b-3b39884a27ca")
		)
		(fp_poly
			(pts
				(xy 2.0415 -4.0635) (xy 2.7585 -4.0635) (xy 2.7585 -2.7865) (xy 2.0415 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "9e01e8db-a157-47f6-8fbb-6ab41a6cb5fe")
		)
		(fp_poly
			(pts
				(xy 2.8415 -4.0635) (xy 3.5585 -4.0635) (xy 3.5585 -2.7865) (xy 2.8415 -2.7865)
			)
			(stroke
				(width 0.01)
				(type solid)
			)
			(fill yes)
			(layer "F.Mask")
			(uuid "db90dfeb-c6fa-45ff-bddc-34917cf85ed4")
		)
		(fp_line
			(start -4.62 -0.27)
			(end -4.62 -1.63)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1f7683b5-b603-4c9f-b37e-b7e8bd1aa1ac")
		)
		(fp_line
			(start -4.62 3.4)
			(end -4.62 2.57)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "62f710f0-4f8a-4dcb-9dcc-2ca885699db2")
		)
		(fp_line
			(start 4.62 -1.63)
			(end 4.62 -0.27)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "44ecd5c3-baf9-42fb-9b29-4b8871016247")
		)
		(fp_line
			(start 4.62 2.57)
			(end 4.62 3.4)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3ce4856a-14b8-4456-9ee9-169bb7657612")
		)
		(fp_line
			(start 4.62 3.4)
			(end -4.62 3.4)
			(stroke
				(width 0.15)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a3dce8b-1b47-4c3f-8d47-c3e5fca71752")
		)
		(fp_line
			(start -5.12 -4.3)
			(end 5.12 -4.3)
			(stroke
				(width 0.01)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "981de380-848e-4143-9280-50b78a9c25de")
		)
		(fp_line
			(start -5.12 3.55)
			(end -5.12 -4.3)
			(stroke
				(width 0.01)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dc7e5e86-5fbf-4c8b-a636-3b110fe5808e")
		)
		(fp_line
			(start 5.12 -4.3)
			(end 5.12 3.55)
			(stroke
				(width 0.01)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3346908a-944f-43ad-93e1-dbe3a58d879e")
		)
		(fp_line
			(start 5.12 3.55)
			(end -5.12 3.55)
			(stroke
				(width 0.01)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "35c2bd16-2d5f-4a5e-ba09-aa06d2716b23")
		)
		(fp_line
			(start -4.47 -3.25)
			(end 4.47 -3.25)
			(stroke
				(width 0.13)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "15572000-d5a5-4397-993a-456e68842eee")
		)
		(fp_line
			(start -4.47 3.25)
			(end -4.47 -3.25)
			(stroke
				(width 0.13)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "aa124276-5045-4783-90b9-7329e8b55187")
		)
		(fp_line
			(start 4.47 -3.25)
			(end 4.47 3.25)
			(stroke
				(width 0.13)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e528dcf6-b0cd-401c-a3a1-90c7b60f7fed")
		)
		(fp_line
			(start 4.47 3.25)
			(end -4.47 3.25)
			(stroke
				(width 0.13)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "f62b97a0-8a57-4f2e-a22f-0ce39097adb0")
		)
		(fp_text user "PTH Slot 0.6 +/-0.05 X 1.8 +/-0.05"
			(at -5.736 -8.998 0)
			(layer "Dwgs.User")
			(uuid "bc498093-3006-40c1-9287-332c84468a39")
			(effects
				(font
					(size 0.393701 0.393701)
					(thickness 0.15)
				)
			)
		)
		(fp_text user "PTH Slot 0.6 +/-0.05 X 1.4 +/-0.05"
			(at -5.686 -7.878 0)
			(layer "Dwgs.User")
			(uuid "4e1a4308-a4fd-43ec-908e-77124be0b8cd")
			(effects
				(font
					(size 0.393701 0.393701)
					(thickness 0.15)
				)
			)
		)
		(pad "A1B12" smd rect
			(at -3.2 -3.425)
			(size 0.59 1.15)
			(layers "F.Cu" "F.Paste")
			(uuid "346ffe9b-beba-4090-bff4-9ffc22dc12ed")
		)
		(pad "A4B9" smd rect
			(at -2.4 -3.425)
			(size 0.59 1.15)
			(layers "F.Cu" "F.Paste")
			(uuid "80a2c160-f346-47d4-87ae-8ddbe73bc468")
		)
		(pad "A5" smd rect
			(at -1.25 -3.425)
			(size 0.298 1.15)
			(layers "F.Cu" "F.Paste")
			(net "Net-(J1-CC1)")
			(pinfunction "CC1_A5")
			(pintype "bidirectional")
			(uuid "8799eb17-d141-43c3-b345-22157de5840c")
		)
		(pad "A6" smd rect
			(at -0.25 -3.425)
			(size 0.298 1.15)
			(layers "F.Cu" "F.Paste")
			(net "unconnected-(J1-D+-PadA6)")
			(pinfunction "D+_A6")
			(pintype "bidirectional+no_connect")
			(uuid "15d43cf6-b749-4479-8dfb-5477b28f2517")
		)
		(pad "A7" smd rect
			(at 0.25 -3.425)
			(size 0.298 1.15)
			(layers "F.Cu" "F.Paste")
			(net "unconnected-(J1-D--PadA7)")
			(pinfunction "D-_A7")
			(pintype "bidirectional+no_connect")
			(uuid "9d4aedd4-37e1-40c7-b5ee-4c663d902874")
		)
		(pad "A8" smd rect
			(at 1.25 -3.425)
			(size 0.298 1.15)
			(layers "F.Cu" "F.Paste")
			(net "unconnected-(J1-SBU1-PadA8)")
			(pinfunction "SBU1_A8")
			(pintype "bidirectional+no_connect")
			(uuid "e9a48f06-3cce-419e-9f89-2104395945c1")
		)
		(pad "B1A12" smd rect
			(at 3.2 -3.425)
			(size 0.59 1.15)
			(layers "F.Cu" "F.Paste")
			(uuid "18d245c1-59d4-4c57-ac6a-6a2d37229418")
		)
		(pad "B4A9" smd rect
			(at 2.4 -3.425)
			(size 0.59 1.15)
			(layers "F.Cu" "F.Paste")
			(uuid "fc7ce863-e974-4955-b043-ac04c1f581cd")
		)
		(pad "B5" smd rect
			(at 1.75 -3.425)
			(size 0.298 1.15)
			(layers "F.Cu" "F.Paste")
			(net "Net-(J1-CC2)")
			(pinfunction "CC2_B5")
			(pintype "bidirectional")
			(uuid "f72b2eee-7e3c-4218-baa4-c36a622aaf6b")
		)
		(pad "B6" smd rect
			(at 0.75 -3.425)
			(size 0.298 1.15)
			(layers "F.Cu" "F.Paste")
			(net "unconnected-(J1-D+-PadB6)")
			(pinfunction "D+_B6")
			(pintype "bidirectional+no_connect")
			(uuid "55c1b6e4-9444-4d97-9add-f2f485528dde")
		)
		(pad "B7" smd rect
			(at -0.75 -3.425)
			(size 0.298 1.15)
			(layers "F.Cu" "F.Paste")
			(net "unconnected-(J1-D--PadB7)")
			(pinfunction "D-_B7")
			(pintype "bidirectional+no_connect")
			(uuid "4fa4066e-abd0-42d3-8e20-9f98576be4f9")
		)
		(pad "B8" smd rect
			(at -1.75 -3.425)
			(size 0.298 1.15)
			(layers "F.Cu" "F.Paste")
			(net "unconnected-(J1-SBU2-PadB8)")
			(pinfunction "SBU2_B8")
			(pintype "bidirectional+no_connect")
			(uuid "aa327154-edac-4c7f-9b93-9a902972e4b7")
		)
		(pad "SH1" thru_hole oval
			(at -4.32 1.15)
			(size 1 2.2)
			(drill oval 0.6 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0762)
			(uuid "97d25e92-b6d1-4a6a-8733-77d3590e0482")
		)
		(pad "SH2" thru_hole oval
			(at 4.32 1.15)
			(size 1 2.2)
			(drill oval 0.6 1.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0762)
			(uuid "a8800411-6fcd-42c1-8ab2-d8108a53c08c")
		)
		(pad "SH3" thru_hole oval
			(at -4.32 -2.85)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0762)
			(uuid "ec3cf1e9-1864-4b79-8d5b-f07518d2dd85")
		)
		(pad "SH4" thru_hole oval
			(at 4.32 -2.85)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(solder_mask_margin 0.0762)
			(uuid "df725306-6069-44fa-9c28-522dfd7645e9")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "26bdb503-9b99-41a9-9e37-83492f9412c3")
		(at 104.715 53.105)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "c5bf6bfa-9975-4a8b-925c-96c44cfeb3a2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "9fe0ab9b-f51b-4b4d-9c0b-e98f704d8093")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fec7656f-9ff0-47bc-a811-fbcfa300780c")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "911ffdd0-9f40-4030-aa6e-9495ca3cd4ca")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a18b6527-b047-4553-8fcd-cdbfe27bc2a3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/e3c39e4c-4a7d-449c-b3e3-b7a87cdb135f")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "0dee91a2-4e3a-4926-ba1c-67dd798616d9")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "a762f70c-24e1-47a0-aeb9-c246f68552df")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "18c19d84-8b95-4714-ae1e-48010e71d60a")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "e24c06cf-001d-4134-9638-a242a957e494")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "f4211231-c4e6-4ddc-942f-42c61a6a9bd5")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J2-RCT)")
			(pintype "passive")
			(uuid "db572d0b-b07f-4e09-88f1-940ca55889d1")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "ad5aed62-f41f-4c41-9ef7-e8e5e0702369")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-563"
		(layer "F.Cu")
		(uuid "2e828881-bcf7-48da-85cd-2c1804eb53fb")
		(at 116.305 62.4)
		(descr "SOT, 6 Pin (https://www.jedec.org/system/files/docs/MO-293B.pdf)")
		(tags "SOT TO_SOT_SMD JEDEC-MO-293-UAAD Texas-DRL-6")
		(property "Reference" "IC2"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(uuid "a7cb4222-6f68-45c0-928b-b07739794fd5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "TPS62A06ADRLR"
			(at 0 1.65 0)
			(layer "F.Fab")
			(uuid "4ed0394e-9409-4833-9c01-8e0d66fd6047")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "183da876-349b-4bde-8cd6-44a226280e9d")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Switching Voltage Regulators 2.5-V to 5.5-V input, 1-A high-efficiency step-down converter with forced PWM in SOT-563 package"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "46f81a96-e39d-49bf-befe-a519adc77b0a")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "package/gullwing"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "d72dea30-192e-4bfa-b1cb-9e5784d0033c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Height" "0.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "5149c4cb-fed5-4ae2-813b-19edb2674b6a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" "TPS62A06ADRLR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "d2ff51a3-b54b-4368-af46-50f06e398d5d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4579d288-f63f-48a0-b043-115db9da7bcb")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Texas Instruments"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "cea0ccbd-9f34-441e-8fd7-93db33ebc9b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "TPS62A06ADRLR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "90a74722-b5d9-4b81-a75b-4c773e1d6c53")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/5ed6d843-1a99-4598-b0d3-adb45d89259b")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "3" "4" "1" "2" "6" "5")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.425568 -0.935)
			(end 0.71 -0.935)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9a43072a-699a-46ee-8ddf-01ee0e55146b")
		)
		(fp_line
			(start 0.71 0.935)
			(end -0.71 0.935)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d576627a-3f3a-449c-a070-8052561948bb")
		)
		(fp_poly
			(pts
				(xy -0.72 -0.94) (xy -0.86 -1.13) (xy -0.58 -1.13)
			)
			(stroke
				(width 0.12)
				(type solid)
			)
			(fill yes)
			(layer "F.SilkS")
			(uuid "a151fd62-98c8-42e3-9178-34557fc74eda")
		)
		(fp_line
			(start -1.2 -0.83)
			(end -0.75 -0.83)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bc969c46-2c40-4437-8433-9d45bbdc4117")
		)
		(fp_line
			(start -1.2 0.83)
			(end -1.2 -0.83)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "af092101-e040-42fc-86bd-cadffb474beb")
		)
		(fp_line
			(start -0.75 -0.95)
			(end 0.75 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "10ae878f-e7da-42b5-88b8-0b491c758832")
		)
		(fp_line
			(start -0.75 -0.83)
			(end -0.75 -0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7e5320cb-80a7-4ac9-8bf9-81ae62ef6c93")
		)
		(fp_line
			(start -0.75 0.83)
			(end -1.2 0.83)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "14454f8f-540a-4b1c-be3f-6cad8a753864")
		)
		(fp_line
			(start -0.75 0.95)
			(end -0.75 0.83)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "382829c8-6c8f-46be-ae21-269f89ae1f45")
		)
		(fp_line
			(start 0.75 -0.95)
			(end 0.75 -0.83)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "bd7db989-00e6-49b5-ba16-d4f8bfddd7b8")
		)
		(fp_line
			(start 0.75 -0.83)
			(end 1.2 -0.83)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ef8b7a19-49da-4bee-a3a4-e6b3ea676182")
		)
		(fp_line
			(start 0.75 0.83)
			(end 0.75 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fa99a927-bcd9-43a6-878c-9be889a3305d")
		)
		(fp_line
			(start 0.75 0.95)
			(end -0.75 0.95)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a437ae0c-b42e-452e-ab20-634d4b7f07d9")
		)
		(fp_line
			(start 1.2 -0.83)
			(end 1.2 0.83)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "65883318-0afb-41ac-a30b-5eab170ed16c")
		)
		(fp_line
			(start 1.2 0.83)
			(end 0.75 0.83)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "5e85249c-fee1-4372-be7b-ba474106e962")
		)
		(fp_poly
			(pts
				(xy -0.3 -0.8) (xy 0.6 -0.8) (xy 0.6 0.8) (xy -0.6 0.8) (xy -0.6 -0.5)
			)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "cd3a3e58-0bf6-4e84-91f0-5f34f8d66288")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
			(uuid "28a0526b-fd6a-4818-ad3e-d7e910989066")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.7125 -0.5)
			(size 0.675 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_1")
			(pintype "passive")
			(uuid "c7411c98-15cf-47f4-b3f7-c57ca5a0525f")
		)
		(pad "2" smd roundrect
			(at -0.7125 0)
			(size 0.675 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(IC2-SW)")
			(pinfunction "SW_2")
			(pintype "passive")
			(uuid "b6305690-1956-457a-8218-96be79ff95eb")
		)
		(pad "3" smd roundrect
			(at -0.7125 0.5)
			(size 0.675 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VBUS")
			(pinfunction "VIN_3")
			(pintype "passive")
			(uuid "efcd32a2-2f9a-496b-93cc-96c2fa27428b")
		)
		(pad "4" smd roundrect
			(at 0.7125 0.5)
			(size 0.675 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VBUS")
			(pinfunction "EN_4")
			(pintype "passive")
			(uuid "058a56fe-0d95-46ba-b961-f20a67f40c13")
		)
		(pad "5" smd roundrect
			(at 0.7125 0)
			(size 0.675 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(IC2-FB)")
			(pinfunction "FB_5")
			(pintype "passive")
			(uuid "0b7250ba-3be3-48d5-9222-61705504374d")
		)
		(pad "6" smd roundrect
			(at 0.7125 -0.5)
			(size 0.675 0.35)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "unconnected-(IC2-PG-Pad6)")
			(pinfunction "PG_6")
			(pintype "passive+no_connect")
			(uuid "ee7ac712-aee7-4bc5-b601-3d6c231fc25b")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-563.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "32bb3e6e-8b81-460f-ae44-574d1dbc4a0e")
		(at 100.705 63.145)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "5246148b-b9be-4509-87f8-f60a451e2b2a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22μF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "75f06fa3-024f-47a0-9de6-b4cc89da0ab2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0d514e04-ea44-46f2-b254-a33a9160c06c")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "acd9f4d1-de31-479e-baab-1023fb5a1fc5")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "be9c069b-c2ce-420a-8797-2677ce4fa699")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/c65b603a-dbec-4610-83d2-1675a6934745")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5e624590-3d49-4e41-b96f-e8652096cb2c")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5de52ef2-b245-4781-80d8-29a9b0076cf4")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "4af63f4a-da52-46e4-b83a-37f8c76ded0f")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "70343395-6f92-4764-83f3-56edb245ab80")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "8ab2ec7a-acde-4546-8692-43b886bf0986")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3.3V")
			(pintype "passive")
			(uuid "3b131556-36fe-4161-beb4-940f18138ccf")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "5c6e7a12-2556-4d8a-9aec-59885ba25da7")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "337105b3-5a6c-433f-9a97-9f8c22993435")
		(at 100.705 60.635)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "c0afdca2-8068-4275-90ac-2093068655ed")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22μF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "e1984f92-731c-49f6-9311-0053967b295b")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e0eb90a3-afaa-4a56-8518-bbb7bd0c003a")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "c2a6c808-72b7-45fd-ad26-852c38618090")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "1895fead-5210-42d7-af53-56253b526fe9")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5773ed54-e39c-4309-a5b9-22520fe8d69a")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12c7f346-910c-4443-ace7-d795b823b7b6")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "07b342db-9e68-40fa-adf6-5220f5fc7037")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "8a7d5110-f605-49f8-ba9c-03e020710727")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "38e951f7-6ef2-4f30-8f75-e0c77be37332")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "c8679723-5e3d-439d-9c3c-fe1e0111fade")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3.3V")
			(pintype "passive")
			(uuid "7259cf46-4e37-44d5-885c-de962c6bc73b")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "886c01f1-8b60-482c-a5d0-1e9efc6aa956")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "4e5b1ede-b36b-45d0-baef-4b0bdcb20d1b")
		(at 100.705 53.105)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "fd49b1df-1793-4261-a1c4-d9ae47412b37")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22μF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "196d19c6-b5e2-4caf-8312-5575e5d712f2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "422a4033-05c7-4d24-bdc4-7cc08ab5d6f6")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "fd4c7810-b453-4dd4-b88e-74ef9444f5c3")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "596c188f-ceb3-40a8-8605-2802d38b0bfa")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/553601db-4780-40d5-adcc-029384330a42")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "bb161fc8-2979-46bd-a3de-5fe5a6adb39a")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9f986525-b4ee-441e-88b3-ed1310ddc151")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "ec08e3f2-5130-40ff-86fb-c68679b7cfe9")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "fd6749a7-55e4-4007-912f-4f0fcdb36b9e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7f3dd321-f2f3-45f3-8442-82b03e47df50")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VBUS")
			(pintype "passive")
			(uuid "bf3be888-6e75-4501-8280-198584cad898")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "350ffa9f-4515-4e73-985c-ad91e2493a8a")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "5d7a2918-e516-41d8-a35a-5625dcaef9f4")
		(at 104.715 63.145)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f90ed9c1-4f9f-4c74-875f-c38aae6e3ba4")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "640246ad-7d37-4b40-8675-fba59c97e833")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c28a016-a0d0-4183-8de0-dedae3dca969")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7c1d93a9-9224-4d10-aab8-70e46ed591a6")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "03ce5fcf-f4cb-4b18-b403-8bc6b053e621")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/d43323ce-e732-41f8-b5c3-e28d2ffde488")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4a142242-8863-4a5c-9ebf-391cf25184d4")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "12bff480-cb8e-4d9b-8ae5-20176ec13988")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "26ba1310-a020-4ae4-b69e-1769551b66df")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "a1e1af24-0592-4093-ac13-60b7ce6c7cc1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "4c3965f1-0393-41fd-b51f-c22d590fc675")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J4-RCT)")
			(pintype "passive")
			(uuid "4ba2389b-fa7d-4baf-97f3-89e5c7af1f28")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "bced3670-f79c-4a60-9a26-543c593d6571")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(uuid "6ecf1ff3-d076-443c-957e-944baf6d37f7")
		(at 108.175 65.685)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(uuid "c304d2a0-0947-4558-b077-0cad90b07cfe")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "453k"
			(at 0 1.17 0)
			(layer "F.Fab")
			(uuid "92c9b42d-3b08-40fd-8b63-8a03a10ea99f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "163ff3c4-6eab-4fe2-9c62-0a7b6009021b")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "0b262563-b0ed-435f-8c4b-c9c4c8ba003f")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "fa7481c5-36f3-4f7a-b5e9-369fd1c99103")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/7c75a813-7bd7-4143-b157-25509760d752")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.153641 -0.38)
			(end 0.153641 -0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f2f70e20-210b-408f-a868-fb2ff84174b8")
		)
		(fp_line
			(start -0.153641 0.38)
			(end 0.153641 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "de3ad8c5-20d4-4f38-aa25-56f714c58c1e")
		)
		(fp_rect
			(start -0.93 -0.47)
			(end 0.93 0.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "4e05f81f-6e15-442a-99d9-f0aa5a46368f")
		)
		(fp_rect
			(start -0.525 -0.27)
			(end 0.525 0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "22601282-1a8c-4661-a9fc-001290aeb80e")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "5b83c906-2d1a-44d5-a575-a486759309ac")
			(effects
				(font
					(size 0.26 0.26)
					(thickness 0.04)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3.3V")
			(pintype "passive")
			(uuid "c64f7389-2b78-47ee-8faf-6a9b46144d98")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(IC2-FB)")
			(pintype "passive")
			(uuid "74f88aba-2f0f-4190-9c3e-83399a1a2772")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "726fcd6b-fbf4-4a76-9d78-5abd1612808c")
		(at 100.705 55.615)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "347dfd58-d828-4d49-a3d5-cbf173845e98")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22μF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "a6760005-911f-4a76-abb0-db6aa007cc91")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "3941a366-64e7-47e5-97b6-ed45a943f810")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8c9401fd-975c-4c60-aef7-9371cb427380")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5cf4c134-35e9-4906-85f4-a534b05847dc")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/5551f939-7a7d-4583-9b74-4aa186bdfd5e")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "51b983fd-40ad-484b-9119-5d8943ede44b")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "3dea4886-3146-4ab8-9963-cc8012eeed8d")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "5c1c2698-4217-482e-9709-fdb7dfba8f56")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "11e7c67d-c1eb-45e3-8837-64b3d0f928c1")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a12080e7-dbe0-4f4b-b45d-dc950b3587da")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "VBUS")
			(pintype "passive")
			(uuid "aedb49bc-0589-4cbc-97d8-91513af9ab7a")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "9286f6bd-206d-46c9-8ef7-1aaaad25cd02")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(uuid "72db209b-0ee7-4bc7-ad33-975469a75e5a")
		(at 108.175 61.705)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(uuid "c4548e55-7dbe-4837-8c06-0042f8f17646")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "5.1k"
			(at 0 1.17 0)
			(layer "F.Fab")
			(uuid "dcfe653a-f2df-4cae-b5d8-41c8a2dc5dcd")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "e62d5f57-b97e-4a28-8a5e-311a2ad330a0")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a840fd59-2dfb-4ccf-9f39-bca324d81817")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "ff505789-ff59-4823-8435-ddb7e1ddb885")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/afe60e16-3f89-41f6-8f88-318fea1ec892")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.153641 -0.38)
			(end 0.153641 -0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "daa923a6-d4a6-4049-bfc3-67fa983c5674")
		)
		(fp_line
			(start -0.153641 0.38)
			(end 0.153641 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8ce45232-9d28-4b97-ba33-7293d8708def")
		)
		(fp_rect
			(start -0.93 -0.47)
			(end 0.93 0.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "2c04187c-0ee7-4b8a-8022-f033041b1351")
		)
		(fp_rect
			(start -0.525 -0.27)
			(end 0.525 0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "508757a9-6577-4b44-a9bc-14e2fccfd96c")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "a50eef91-6eb4-4b18-a59b-83779d9e71ce")
			(effects
				(font
					(size 0.26 0.26)
					(thickness 0.04)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J1-CC2)")
			(pintype "passive")
			(uuid "efef1e21-7545-44d6-baf3-bb520c5c04c1")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "33adca1f-9515-4759-b2a4-955ea198cc77")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "7b0ab2c1-4eef-45ac-9814-d989b2b763ba")
		(at 100.705 58.125)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "a361b353-20eb-413f-a912-28b33122ded2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "22μF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "39dd0ac2-5832-459b-925b-dc5994eeaba7")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "48ffcb2a-a2d9-4187-b5e8-d69363da5a26")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "585d8ee6-c5d9-482f-a44d-25844480ec73")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "b1661cea-68cc-46df-89bb-237134bd4867")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/11057f7e-eb07-40df-837c-27709b3ca4d4")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d25895b1-1e0a-4432-a741-6e7c5ebda527")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "899b4b27-115a-42b3-8aa3-ef2ce76e1c89")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "3890fa1b-d8d6-4095-852c-53befb72a34c")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "53984f10-4efc-4511-9284-82c7057552e7")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "3c2386a2-d5cb-4898-9458-a56dc7517528")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3.3V")
			(pintype "passive")
			(uuid "4db1e7e0-1bf4-4314-90de-e80c48a4ec46")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "06f3464a-ae48-4523-a254-73ff9fa4ed88")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "945f4249-778c-45c1-a19e-1399acea55c7")
		(at 104.715 58.125)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "81ff2576-d27a-4073-9cfa-170542e1a564")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "2e74cd37-d00f-4da8-9e39-ba1d06723cf8")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "77b1f768-0bde-42be-931f-c7101b4f7cf1")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "faaa735a-c636-40cf-b97f-c40328777e23")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "5ae74205-2179-4c83-86a6-233b85164e19")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/6f0003b4-4520-430f-bd7d-a1be1f1bdc57")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d095c510-a7b9-4451-bd1a-ab625ce91994")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "059397e6-f5ef-4dfb-beaa-cd41851cfd96")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "f04c9c1f-3941-4531-b0e7-98823a23f7cc")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "8ef6e1d4-dc55-4d99-8175-c2ac2d347f2f")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e48c259e-fada-475d-a51a-f74068b4dbc5")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J3-RCT)")
			(pintype "passive")
			(uuid "fbf433d4-7e73-4986-9181-a1333786b102")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "62854449-aa9e-4add-bc74-44cf5871bbe3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "99902107-3c0f-411e-99f3-1593adad5ffc")
		(at 100.705 65.655)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "f1bb31bb-f0ef-462b-97da-b9c336f6677f")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "c7424ef7-1ed2-4faf-92be-0feb74f41f28")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ed980b12-af2f-4ba0-98d8-b929957fc629")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5904ac15-62d9-4ceb-b825-e4bfb0b89309")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "17866793-01e9-496e-a7f8-2c92a9780d49")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/501ca411-1335-4e67-887c-4c2e9d84f7c3")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c9009c0b-8ed4-40bc-ba25-cf7be3c35dd1")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5ebf3b59-367e-43cd-ae78-67d416b0b228")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "3ae667e4-36e9-4140-bd6f-5cd438e19c32")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "5bd753c6-75a0-440c-870a-e8402cf3eb95")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "87c17195-89ca-4768-9c5e-2c717c43d8a2")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J2-TCT)")
			(pintype "passive")
			(uuid "09855362-d9d4-4a3b-8115-b6b2a50916de")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "6cba2dea-2cd3-411e-88cb-ddee8501df14")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_RJ:RJ45_Hanrun_HR911105A_Horizontal"
		(layer "F.Cu")
		(uuid "af499b0c-b131-4cb6-a9d2-2fd72fc541fe")
		(at 65.085 33.565)
		(descr "1 Port RJ45 8P8C receptacle, shielded, with magnetics, through hole, 2 LEDs, tab down, http://www.hanrun.com/public/upload/down/2020/09-11/cc11be56d66bb63d5f1eeb85492439c0.pdf")
		(tags "RJ45 Magjack ethernet")
		(property "Reference" "J2"
			(at 4.44 -5 0)
			(layer "F.SilkS")
			(uuid "80358c84-1d37-4d35-8c7d-bf6bc3f0d97a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RJ45_Hanrun_HR911105A_Horizontal"
			(at 4.44 18.5 0)
			(layer "F.Fab")
			(uuid "d474ee19-8da1-4d2f-8006-bdaa4ca2323a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141815_HANRUN-Zhongshan-HanRun-Elec-HR911105A_C12074.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "27626be0-d230-4cbf-b4a8-218ca92d58f8")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "fbd58076-981b-4064-a36d-bdc56fc8f216")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "RJ45*Hanrun*HR911105A*")
		(path "/091c5eea-e5c5-4860-b04e-e505f565cbc4")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "4" "2" "3" "5" "6" "8" "SH" "7" "12" "11" "9" "10")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -3.92 -0.9)
			(end -3.92 0.9)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "240659b4-17e9-4814-9c26-8aacde5305dc")
		)
		(fp_line
			(start -3.69 -4.15)
			(end -3.69 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c03b701e-9097-4ed7-80f8-15adefc6d081")
		)
		(fp_line
			(start -3.69 -4.15)
			(end 12.57 -4.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c1ed74a7-f05f-47da-bd46-aba5e045c53e")
		)
		(fp_line
			(start -3.69 4.93)
			(end -3.69 11.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "adf28c9b-66cb-4356-87f6-ae79672a65f3")
		)
		(fp_line
			(start 12.57 -4.15)
			(end 12.57 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "53ac88ae-babc-4aba-832f-1d9eb3ada318")
		)
		(fp_line
			(start 12.57 4.93)
			(end 12.57 11.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4e1ef19-66e9-4295-b8dd-37031e126eba")
		)
		(fp_line
			(start -5.06 2.57)
			(end -5.06 4.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "233f521c-58fa-430d-81e9-4b0d23d8261c")
		)
		(fp_line
			(start -5.06 2.57)
			(end -4.08 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "a5a798c2-4da1-42c1-99e5-8a58377d10bc")
		)
		(fp_line
			(start -5.06 4.05)
			(end -4.08 5.03)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "22119d8c-f4ce-48d9-ae91-7075be788422")
		)
		(fp_line
			(start -4.08 -4.54)
			(end -4.08 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ecdd7c85-8473-42c0-930e-a2a63ee0b749")
		)
		(fp_line
			(start -4.08 -4.54)
			(end 12.96 -4.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ca0a0fab-63be-4c13-b9f4-0b1d3d962e3c")
		)
		(fp_line
			(start -4.08 5.03)
			(end -4.08 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "97cada59-9f7c-47ec-b729-81d65dddc10a")
		)
		(fp_line
			(start -4.08 17.76)
			(end 12.96 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b3ae7bbc-f1cd-4739-bed3-ff7f3475f73f")
		)
		(fp_line
			(start 12.96 -4.54)
			(end 12.96 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "64351d8d-e288-4b9e-a668-184994ff4958")
		)
		(fp_line
			(start 12.96 5.03)
			(end 12.96 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ddf522cb-324b-4852-a4d7-de39ae19e08c")
		)
		(fp_line
			(start 13.94 2.57)
			(end 12.96 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "b8232e45-de76-4b4f-8f3b-5f33ed251efe")
		)
		(fp_line
			(start 13.94 4.05)
			(end 12.96 5.03)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "fe4e3666-8557-4441-902d-191b756b7b6e")
		)
		(fp_line
			(start 13.94 4.05)
			(end 13.94 2.57)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "461a03a4-e612-45a3-943e-44b0ac08657e")
		)
		(fp_line
			(start -3.58 -4.04)
			(end -3.58 -1.01)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "49f7d66b-f8bd-42d6-a9f8-eaa728a84677")
		)
		(fp_line
			(start -3.58 -4.04)
			(end 12.46 -4.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3413b806-0884-4759-b02e-71c7d5a5b706")
		)
		(fp_line
			(start -3.58 0.99)
			(end -3.58 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "5e89f332-617b-4924-8925-2fb033cd578e")
		)
		(fp_line
			(start -3.58 17.26)
			(end 12.46 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "8848c0e4-ae64-42ce-b529-b7ccec251e35")
		)
		(fp_line
			(start -2.58 -0.01)
			(end -3.58 -1.01)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "80c9586e-5f06-4bd7-af5a-5a64ca3a1a18")
		)
		(fp_line
			(start -2.58 -0.01)
			(end -3.58 0.99)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "69bb1203-f92d-4cda-8a66-a1cd43a02364")
		)
		(fp_line
			(start 12.46 -4.04)
			(end 12.46 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "885393c0-2d34-4a37-900f-007d7f4aa195")
		)
		(fp_text user "${REFERENCE}"
			(at 4.44 6.36 0)
			(layer "F.Fab")
			(uuid "3674d7c5-8347-4f82-a6b3-4a0751ee8221")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -1.275 6.36)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(uuid "c05872ec-0803-4f8a-8ec5-738d9947ccbc")
		)
		(pad "" np_thru_hole circle
			(at 10.155 6.36)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(uuid "a56adafd-1872-4610-97eb-1575d56407df")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.167)
			(net "MDI_TP_P0")
			(pinfunction "TD+_1")
			(pintype "passive")
			(uuid "1cfb181b-5b3f-4d3d-9408-7960f3f2b7d7")
		)
		(pad "2" thru_hole circle
			(at 1.26 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_TN_P0")
			(pinfunction "TD-_2")
			(pintype "passive")
			(uuid "21786f6d-fae8-47e4-bb95-ea2308f1f68d")
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_RP_P0")
			(pinfunction "RD+_3")
			(pintype "passive")
			(uuid "9f234ca1-c3d2-4909-9078-25118b76f9b4")
		)
		(pad "4" thru_hole circle
			(at 3.8 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-TCT)")
			(pinfunction "TCT_4")
			(pintype "passive")
			(uuid "309ab02c-ddee-459b-88a4-fa8f85f9a22f")
		)
		(pad "5" thru_hole circle
			(at 5.08 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J2-RCT)")
			(pinfunction "RCT_5")
			(pintype "passive")
			(uuid "e750a9cb-6ce2-4754-abf0-893e2c5351db")
		)
		(pad "6" thru_hole circle
			(at 6.34 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_RN_P0")
			(pinfunction "RD-_6")
			(pintype "passive")
			(uuid "b4d755aa-296a-4b91-befd-6a37a0ac6075")
		)
		(pad "7" thru_hole circle
			(at 7.62 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J2-NC-Pad7)")
			(pinfunction "NC_7")
			(pintype "no_connect")
			(uuid "76924ec2-388a-4575-88ab-bcc9098c8117")
		)
		(pad "8" thru_hole circle
			(at 8.88 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "power_in")
			(uuid "17b81590-2c26-4e9e-8f11-d5d4a3e7bd0f")
		)
		(pad "9" thru_hole circle
			(at -2.185 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J2-Pad9)")
			(pintype "passive")
			(uuid "9ac17cef-0eed-4da9-b73e-20bca272bf53")
		)
		(pad "10" thru_hole circle
			(at 0.355 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J2-Pad10)")
			(pintype "passive")
			(uuid "01ad8c04-6a41-4c85-99fc-1372e7ad63c0")
		)
		(pad "11" thru_hole circle
			(at 8.525 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J2-Pad11)")
			(pintype "passive")
			(uuid "09cd121b-2af8-4eaf-90e8-8de38f967fc4")
		)
		(pad "12" thru_hole circle
			(at 11.065 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J2-Pad12)")
			(pintype "passive")
			(uuid "26119723-f9da-4171-9dfd-efe4cc5e0574")
		)
		(pad "SH" thru_hole circle
			(at -3.305 3.31)
			(size 2.5 2.5)
			(drill 1.63)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
			(uuid "c32d9097-b6f9-44e2-a9b8-de87a274ddaa")
		)
		(pad "SH" thru_hole circle
			(at 12.185 3.31)
			(size 2.5 2.5)
			(drill 1.63)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
			(uuid "650b13dc-d7bd-45e4-91cf-d71c5d602f12")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Hanrun_HR911105A_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "b84f17e6-a2ef-4fac-b866-5431840df2c5")
		(at 104.715 55.615)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "17b15a85-bafc-488e-9786-39a4fabe145a")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "5398e7cf-543a-483a-a98b-df2526e5c9a6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "5d6cd84a-dbd4-4fda-9282-02c2fcfcd7fc")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "92fc1324-83a5-4e79-880e-e6ea6d2984c0")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "8d7427c2-1df0-4071-8f52-5126488632f3")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/e3880380-3246-407c-9e5e-583eb1b1d4ad")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "77fd40bc-d82a-4993-9a33-1b74905d3036")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "75bea58f-dfd2-40fb-860e-a2bb368e70a8")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "24feb00b-02ec-404f-825c-7b13d2c0dc3e")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "57c53cc8-75a6-4fd1-8850-bda8e4258a28")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "07b88a32-0350-4a49-af1b-a62863347f91")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J3-TCT)")
			(pintype "passive")
			(uuid "dd416ae5-1c8d-4ac7-a0eb-94f9218ffbe1")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "dd647ca4-86e6-4817-9d66-e65f6857dc62")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1008_2520Metric"
		(layer "F.Cu")
		(uuid "c5ce2b6b-514b-482a-b64c-2a6dde8600cc")
		(at 112.105 62.585)
		(descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf)")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 -2.05 0)
			(layer "F.SilkS")
			(uuid "b8956aed-7015-40e2-a823-b1b19d7e9c67")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "MGV252010R22M-10"
			(at 0 2.05 0)
			(layer "F.Fab")
			(uuid "627418c5-1ecc-491a-8179-d1f5dcafcf04")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "7d7789ce-7267-4f1e-adbc-10ad828e757d")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "8eca4935-6550-4be3-9fc8-f1d95c268739")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "cf130664-ee43-4299-b15f-252ddae19478")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(path "/af27c9e4-7e8d-4f85-81f4-40b582747d81")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.261252 -1.11)
			(end 0.261252 -1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "22c39f4c-0d19-4fdb-a4c8-025906cbcb16")
		)
		(fp_line
			(start -0.261252 1.11)
			(end 0.261252 1.11)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8fbb719f-fc1d-4ae8-9cdf-9efabf024da1")
		)
		(fp_rect
			(start -1.95 -1.35)
			(end 1.95 1.35)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "d64f65c2-6a72-4475-b27d-dce39d0a4b58")
		)
		(fp_rect
			(start -1.25 -1)
			(end 1.25 1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "85a67cd7-77bd-47f2-af5e-e46dfea6f897")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "7e220cf0-7779-4cf9-8352-50e97f1f220d")
			(effects
				(font
					(size 0.62 0.62)
					(thickness 0.09)
				)
			)
		)
		(pad "1" smd roundrect
			(at -1.075 0)
			(size 1.25 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "Net-(IC2-SW)")
			(pinfunction "1_1")
			(pintype "passive")
			(uuid "a5642bc0-0873-4277-bfa9-6496fe13cf1d")
		)
		(pad "2" smd roundrect
			(at 1.075 0)
			(size 1.25 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net "+3.3V")
			(pinfunction "2_2")
			(pintype "passive")
			(uuid "018b0450-2f41-4f2e-b621-93e613b5520f")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(uuid "d12fd656-0941-44fc-a5c6-7648723a3acc")
		(at 108.175 67.675)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.17 0)
			(layer "F.SilkS")
			(uuid "a6d1c36e-c851-4ea1-8be8-5470b126b8ba")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100k"
			(at 0 1.17 0)
			(layer "F.Fab")
			(uuid "50f8cb96-e068-471f-9184-b770caa7e92d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "de4a446a-71d7-476c-83f7-d397455ca10d")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Resistor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "ec925a47-8637-464a-bcb2-fad87f167bc5")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "a635dfcf-6258-4202-b1d8-7a5edb660eaf")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "R_*")
		(path "/fc12ce23-45b4-4223-9f3b-dc9ec68cec7b")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.153641 -0.38)
			(end 0.153641 -0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "40781b6c-21c8-41dd-b684-8389204dd8be")
		)
		(fp_line
			(start -0.153641 0.38)
			(end 0.153641 0.38)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32b30411-952b-4be2-b6b9-31f8e1a5d1cb")
		)
		(fp_rect
			(start -0.93 -0.47)
			(end 0.93 0.47)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "25b7eca4-81a9-4626-99d4-e9f8e300b8bc")
		)
		(fp_rect
			(start -0.525 -0.27)
			(end 0.525 0.27)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "7973f147-5c66-4d6a-a234-a5883fae7020")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "275632fa-fac5-4d97-98f8-8e13ea52a820")
			(effects
				(font
					(size 0.26 0.26)
					(thickness 0.04)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(IC2-FB)")
			(pintype "passive")
			(uuid "04d7c961-a13f-4788-aade-7d4c0cfa712b")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "88f751e8-a2db-49f5-9db4-2db19c766031")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(uuid "db76fc4b-9e78-4d9a-8a17-c2c0e660692a")
		(at 104.715 60.635)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(uuid "b6e19820-7b48-4ef2-8a12-549faba4c818")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "100nF"
			(at 0 1.43 0)
			(layer "F.Fab")
			(uuid "8d60b98a-b7a5-44ca-8297-cc9d73382594")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "a423cd5a-6882-4e18-a390-767a0f2a82f6")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "Unpolarized capacitor, small symbol"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "396a4b10-38bf-4be3-a2fd-b552dbb0b692")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "81d24bfe-7f4a-4527-a122-b35ef1ed13b0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "C_*")
		(path "/6c808486-1bf2-4c56-a405-737cc88f1663")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -0.14058 -0.51)
			(end 0.14058 -0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4e8aaccd-82a2-4831-90f3-16be7c7011f8")
		)
		(fp_line
			(start -0.14058 0.51)
			(end 0.14058 0.51)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "f279c94b-b8a8-472c-992f-873072c41cb7")
		)
		(fp_rect
			(start -1.48 -0.73)
			(end 1.48 0.73)
			(stroke
				(width 0.05)
				(type solid)
			)
			(fill no)
			(layer "F.CrtYd")
			(uuid "68790867-8f51-4ac3-99a3-4f0ff13b5cb3")
		)
		(fp_rect
			(start -0.8 -0.4)
			(end 0.8 0.4)
			(stroke
				(width 0.1)
				(type solid)
			)
			(fill no)
			(layer "F.Fab")
			(uuid "fd2ce5d7-111b-4e48-92f4-ac72ada94149")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
			(uuid "e5095424-dfa9-4a74-b07b-382933519c64")
			(effects
				(font
					(size 0.4 0.4)
					(thickness 0.06)
				)
			)
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J4-TCT)")
			(pintype "passive")
			(uuid "50b82858-3d1d-403a-93a0-ea642788fbd1")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
			(uuid "afa28d85-d31f-4298-9a10-a39c165b5f9b")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "HLK-MT7628N:HLK7628N"
		(layer "F.Cu")
		(uuid "de0f1d7b-2743-4b87-9c29-cd7ef7dbd973")
		(at 79.55 64.5)
		(descr "HLK-7628N-3")
		(tags "Integrated Circuit")
		(property "Reference" "IC1"
			(at -0.45 -0.425 0)
			(layer "F.SilkS")
			(uuid "8a1e3c20-9069-4954-8ef2-b680d506fc73")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Value" "HLK-7628N"
			(at -0.45 -0.425 0)
			(layer "F.SilkS")
			(hide yes)
			(uuid "0151d95a-0ef9-4f8e-8894-621e630b39d2")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/szlcsc/1907260930_HI-LINK-HLK-7628N_C209920.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "578c6441-1a0d-426c-acc4-e8c6e3003a1a")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Description" "WIFI Modules RoHS"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
			(uuid "f724e543-ea1f-4eb5-8ec3-4f813f988481")
			(effects
				(font
					(size 1.27 1.27)
				)
			)
		)
		(property "Height" "2.8"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ac9b0f2f-ffa1-401d-ba30-dccc553370b6")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Name" "Hi-Link"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "db8d441b-92eb-4fd4-8e61-6d73135aab2d")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Manufacturer_Part_Number" "HLK-7628N"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a9488926-b332-4bd1-b2da-aa2d96b189a5")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "ebf2f12d-7c73-46db-ae44-8b19a2c8fc37")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "67ea0d1c-4ecd-4cfb-8f9b-6cfeba3ff909")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Part Number" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "1a98cda8-86b9-4894-86cc-67a88028680e")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "a3597453-a2c9-42b4-9380-23046a68ed77")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(path "/ecbdd588-0e5f-42d6-9b46-06abab619780")
		(sheetname "/DIY_Router/")
		(sheetfile "DIY_Router.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "6" "7" "8" "9" "10" "11" "12" "13" "14" "15"
					"16" "17" "18" "19" "20" "21" "22" "23" "24" "25" "26" "27" "28" "29"
					"30" "31" "32" "33" "34" "35" "36" "37" "38" "39" "40" "41" "42" "43"
					"44" "45" "46" "47" "48" "49" "50" "51" "52" "53" "54" "55" "56" "EP1"
					"EP2" "EP3"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -17.6 -9.35)
			(end -17.6 -9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d4de5165-50a3-4b2e-828b-a0e72e9dd5d2")
		)
		(fp_line
			(start -17.6 -9.35)
			(end -17.6 -7.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "68c5c61e-1f59-49bc-b305-5a035c942efc")
		)
		(fp_line
			(start -17.6 -7.5)
			(end -17.6 -9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2ea92ab5-fcf5-4b43-a9ae-389504592493")
		)
		(fp_line
			(start -17.6 -7.5)
			(end -17.6 -7.5)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8e1aeba1-baeb-4926-84bb-e4f665af5241")
		)
		(fp_line
			(start -17.6 7.25)
			(end -17.6 7.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "01808574-6e4a-41c7-82cf-bce96b6bf584")
		)
		(fp_line
			(start -17.6 7.25)
			(end -17.6 9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "34990a5b-bb14-4c1b-9ef3-f9df2fdeba63")
		)
		(fp_line
			(start -17.6 9.35)
			(end -17.6 7.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "32a87bf5-2b9f-4ef8-ba47-687fdafd4642")
		)
		(fp_line
			(start -17.6 9.35)
			(end -17.6 9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5222cacd-9e8f-4e65-b911-88fbb3e05d7c")
		)
		(fp_line
			(start 14.5 -11.1)
			(end 14.5 -11.1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "1ea2d19e-ab23-4279-b30d-ec5154a961f0")
		)
		(fp_line
			(start 14.5 -11.1)
			(end 14.5 -11.1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "5fd81e0e-78ee-496c-a1da-a89941262ccc")
		)
		(fp_line
			(start 14.5 -11)
			(end 14.5 -11)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c4c5a8b1-e90e-4a80-89fc-e6462d2afbf5")
		)
		(fp_line
			(start 15.5 -9.35)
			(end 15.5 -9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c65a1ddc-25a2-4a65-9e42-088f60e0936e")
		)
		(fp_line
			(start 15.5 -9.35)
			(end 17.6 -9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "76eb7c17-4455-4d81-89d6-ce2600a90dcb")
		)
		(fp_line
			(start 15.5 9.35)
			(end 15.5 9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "63bdef22-48b9-4a1f-a2db-98dafe46ffe0")
		)
		(fp_line
			(start 15.5 9.35)
			(end 17.6 9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "4987b852-5bbc-4b47-baaa-8420c4ef155f")
		)
		(fp_line
			(start 17.6 -9.35)
			(end 15.5 -9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "fe9ee460-8477-446d-a72d-754927cd5492")
		)
		(fp_line
			(start 17.6 -9.35)
			(end 17.6 -9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "550b224c-3975-4e07-978d-31a01250bf07")
		)
		(fp_line
			(start 17.6 -9.35)
			(end 17.6 -9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6a24c40a-779f-4a69-9e61-7fd4e4ea004d")
		)
		(fp_line
			(start 17.6 -9.35)
			(end 17.6 9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "c6949a9d-5b37-4c2a-9367-5349dc2513d1")
		)
		(fp_line
			(start 17.6 9.35)
			(end 15.5 9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "b5719e8a-e864-47d7-9a9e-bb3e52a68339")
		)
		(fp_line
			(start 17.6 9.35)
			(end 17.6 -9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "d8ed3f5f-2af2-4b0f-ae3b-f9a291400733")
		)
		(fp_line
			(start 17.6 9.35)
			(end 17.6 9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "55ebd00c-ec24-431c-adbe-4dc809504709")
		)
		(fp_line
			(start 17.6 9.35)
			(end 17.6 9.35)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "6d66b973-e26a-4d3f-ae4d-4baad2208b7b")
		)
		(fp_arc
			(start 14.5 -11.1)
			(mid 14.55 -11.05)
			(end 14.5 -11)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "231876af-1c77-49a7-9bd1-3ed1eb033aad")
		)
		(fp_arc
			(start 14.5 -11.1)
			(mid 14.55 -11.05)
			(end 14.5 -11)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "9aa5bfa4-294e-4d45-b871-41d333b4c27b")
		)
		(fp_arc
			(start 14.5 -11)
			(mid 14.45 -11.05)
			(end 14.5 -11.1)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "8f846aec-ebcc-4eee-bdca-438cc839cc9d")
		)
		(fp_line
			(start -19.5 -12.1)
			(end 18.6 -12.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "129053d8-12f8-4c3e-a30b-1ea7aaab5fe7")
		)
		(fp_line
			(start -19.5 11.25)
			(end -19.5 -12.1)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "91b80eb8-5acf-4187-a9bd-cabd7a68f8bb")
		)
		(fp_line
			(start 18.6 -12.1)
			(end 18.6 11.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "373ab86b-38d6-4f06-850c-bf6e7ca4d493")
		)
		(fp_line
			(start 18.6 11.25)
			(end -19.5 11.25)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "2425bae1-22e2-4b69-b30f-de568d0b144e")
		)
		(fp_line
			(start -17.6 -9.35)
			(end -17.6 9.35)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "7a513f34-13a5-453e-9082-0f6a7b91aec0")
		)
		(fp_line
			(start -17.6 9.35)
			(end 17.6 9.35)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "0cb4c6c7-6dd7-4a0f-8c03-da8c463caa8c")
		)
		(fp_line
			(start 17.6 -9.35)
			(end -17.6 -9.35)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bf5c463d-1eec-45ef-9b53-79533d4cd7a3")
		)
		(fp_line
			(start 17.6 9.35)
			(end 17.6 -9.35)
			(stroke
				(width 0.2)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "a4202ad6-7d10-442e-89b6-61b1c6b4658c")
		)
		(fp_text user "${REFERENCE}"
			(at -0.45 -0.425 0)
			(layer "F.Fab")
			(uuid "fc7463c8-5565-4200-8559-aa0e80cf18af")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.254)
				)
			)
		)
		(pad "1" smd rect
			(at 14.5 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_1_1")
			(pintype "passive")
			(uuid "e5993ae3-3585-48fe-a88e-7a903c035b8a")
		)
		(pad "2" smd rect
			(at 13.1 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3.3V")
			(pinfunction "3.3VD_1_2")
			(pintype "passive")
			(uuid "9c8425ff-bbc7-47ed-bdeb-31610228f71b")
		)
		(pad "3" smd rect
			(at 11.7 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3.3V")
			(pinfunction "3.3VD_2_3")
			(pintype "passive")
			(uuid "99dc8404-ad0b-4025-ab76-4886a088bff3")
		)
		(pad "4" smd rect
			(at 10.3 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_2_4")
			(pintype "passive")
			(uuid "6bd9fd23-cbc0-418d-ac41-11ae1b7a53d2")
		)
		(pad "5" smd rect
			(at 8.9 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-SPI_CS0-Pad5)")
			(pinfunction "SPI_CS0_5")
			(pintype "passive")
			(uuid "79ea5402-7674-4696-b2f2-9b929b78673a")
		)
		(pad "6" smd rect
			(at 7.5 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-REF_CLK0-Pad6)")
			(pinfunction "REF_CLK0_6")
			(pintype "passive")
			(uuid "44791e8c-76e2-4490-84c3-5d04ddc10947")
		)
		(pad "7" smd rect
			(at 6.1 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-PERST_N-Pad7)")
			(pinfunction "PERST_N_7")
			(pintype "passive")
			(uuid "c39726fa-addb-414a-b30b-02324532a0a8")
		)
		(pad "8" smd rect
			(at 4.7 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-WDT_RST_N-Pad8)")
			(pinfunction "WDT_RST_N_8")
			(pintype "passive")
			(uuid "c4aab0df-2dbc-4166-9779-572df65922ae")
		)
		(pad "9" smd rect
			(at 3.3 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-EPHY_LED4-Pad9)")
			(pinfunction "EPHY_LED4_9")
			(pintype "passive")
			(uuid "3c1a2dec-0008-4bcc-84ff-d86e729d5bcc")
		)
		(pad "10" smd rect
			(at 1.9 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-EPHY_LED3-Pad10)")
			(pinfunction "EPHY_LED3_10")
			(pintype "passive")
			(uuid "6f45ac3f-8ab5-43d7-8516-6d837eb5502e")
		)
		(pad "11" smd rect
			(at 0.5 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-EPHY_LED2-Pad11)")
			(pinfunction "EPHY_LED2_11")
			(pintype "passive")
			(uuid "a75eaed9-41e0-4739-994a-a8bf352a6461")
		)
		(pad "12" smd rect
			(at -0.9 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-EPHY_LED1-Pad12)")
			(pinfunction "EPHY_LED1_12")
			(pintype "passive")
			(uuid "f5d832e4-3819-4013-97fa-8c06cf50a9e0")
		)
		(pad "13" smd rect
			(at -2.3 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-EPHY_LED0-Pad13)")
			(pinfunction "EPHY_LED0_13")
			(pintype "passive")
			(uuid "fa6993c4-b746-42ae-a7b9-5222f0ce3460")
		)
		(pad "14" smd rect
			(at -3.7 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(IC1-PORST_N)")
			(pinfunction "PORST_N_14")
			(pintype "passive")
			(uuid "cd7f6038-1422-4b1c-902d-f7fba5f0c428")
		)
		(pad "15" smd rect
			(at -5.1 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-UART_TXD1-Pad15)")
			(pinfunction "UART_TXD1_15")
			(pintype "passive")
			(uuid "b4041153-daa6-4505-9abc-13e92343dd7f")
		)
		(pad "16" smd rect
			(at -6.5 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-UART_RXD1-Pad16)")
			(pinfunction "UART_RXD1_16")
			(pintype "passive")
			(uuid "1c1708b8-0da5-4cdf-8b32-36970e42b9b5")
		)
		(pad "17" smd rect
			(at -7.9 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-I2S_SDI-Pad17)")
			(pinfunction "I2S_SDI_17")
			(pintype "passive")
			(uuid "f9734e00-af5d-41f3-a6a4-529b151b6998")
		)
		(pad "18" smd rect
			(at -9.3 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-I2S_SDO-Pad18)")
			(pinfunction "I2S_SDO_18")
			(pintype "passive")
			(uuid "afc4c021-b5f6-4293-b49b-c9a509a291b6")
		)
		(pad "19" smd rect
			(at -10.7 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-I2S_WS-Pad19)")
			(pinfunction "I2S_WS_19")
			(pintype "passive")
			(uuid "eb3f28ed-6942-4273-8c1f-990db6c707f8")
		)
		(pad "20" smd rect
			(at -12.1 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-I2S_CLK-Pad20)")
			(pinfunction "I2S_CLK_20")
			(pintype "passive")
			(uuid "0f1b9018-1c69-438f-b710-5e8adb838f1d")
		)
		(pad "21" smd rect
			(at -13.5 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_3_21")
			(pintype "passive")
			(uuid "0ff0ce46-f5b7-4726-8ae8-c6910be1fbf3")
		)
		(pad "22" smd rect
			(at -14.9 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-ANT-Pad22)")
			(pinfunction "ANT_22")
			(pintype "passive+no_connect")
			(uuid "dd35b89c-335b-4305-b00d-914063ca704b")
		)
		(pad "23" smd rect
			(at -16.3 -9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_4_23")
			(pintype "passive")
			(uuid "f72422d8-1c33-4a9a-9bd5-f7c3b8275b94")
		)
		(pad "24" smd rect
			(at -17.6 -6.35 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-I2C_SCLK-Pad24)")
			(pinfunction "I2C_SCLK_24")
			(pintype "passive")
			(uuid "a7359c42-e6f2-4c8c-910e-bddea71650b2")
		)
		(pad "25" smd rect
			(at -17.6 -4.95 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-I2C_SD-Pad25)")
			(pinfunction "I2C_SD_25")
			(pintype "passive")
			(uuid "503a2ad1-5693-46c0-af4e-6034385e3666")
		)
		(pad "26" smd rect
			(at -17.6 -3.55 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-SPI_CS1-Pad26)")
			(pinfunction "SPI_CS1_26")
			(pintype "passive")
			(uuid "99310de5-75f4-476e-bfcd-22b4b073ea16")
		)
		(pad "27" smd rect
			(at -17.6 -2.15 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-SPI_CLK-Pad27)")
			(pinfunction "SPI_CLK_27")
			(pintype "passive")
			(uuid "05957930-2bba-49a3-9d97-12a6b4a4e848")
		)
		(pad "28" smd rect
			(at -17.6 -0.75 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-SPI_MISO-Pad28)")
			(pinfunction "SPI_MISO_28")
			(pintype "passive")
			(uuid "46089d94-ff16-49ae-87d9-f3b2c90d9615")
		)
		(pad "29" smd rect
			(at -17.6 0.65 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-SPI_MOSI-Pad29)")
			(pinfunction "SPI_MOSI_29")
			(pintype "passive")
			(uuid "895ef8ac-4528-48f8-a4dd-578665dc4b7e")
		)
		(pad "30" smd rect
			(at -17.6 2.05 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-GPIO0-Pad30)")
			(pinfunction "GPIO0_30")
			(pintype "passive")
			(uuid "f9eb3845-31a7-499f-8b77-2e714d8d81de")
		)
		(pad "31" smd rect
			(at -17.6 3.45 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-UART_TXD0-Pad31)")
			(pinfunction "UART_TXD0_31")
			(pintype "passive")
			(uuid "182990a3-df90-4ad6-9f15-c1a6931d7d99")
		)
		(pad "32" smd rect
			(at -17.6 4.85 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-UART_RXD0-Pad32)")
			(pinfunction "UART_RXD0_32")
			(pintype "passive")
			(uuid "c13d9c56-dc8f-45ac-ae84-9d9f795588e0")
		)
		(pad "33" smd rect
			(at -17.6 6.25 90)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-WLED_N-Pad33)")
			(pinfunction "WLED_N_33")
			(pintype "passive")
			(uuid "464de2bb-3466-451a-abd7-f1cb9d1f6a71")
		)
		(pad "34" smd rect
			(at -16.3 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_RP_P0")
			(pinfunction "MDI_RP_P0_34")
			(pintype "passive")
			(uuid "e242cc15-2eff-4f93-974e-1882634a6165")
		)
		(pad "35" smd rect
			(at -14.9 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_RN_P0")
			(pinfunction "MDI_RN_P0_35")
			(pintype "passive")
			(uuid "fb1686b9-8677-4f57-90d0-ed22d2739ca7")
		)
		(pad "36" smd rect
			(at -13.5 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_TP_P0")
			(pinfunction "MDI_TP_P0_36")
			(pintype "passive")
			(uuid "bedb9902-3399-4864-9fa1-7826ba6d6a08")
		)
		(pad "37" smd rect
			(at -12.1 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_TN_P0")
			(pinfunction "MDI_TN_P0_37")
			(pintype "passive")
			(uuid "19a7d762-62b3-4bda-8ca4-19bbf8e7a263")
		)
		(pad "38" smd rect
			(at -10.7 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_TP_P1")
			(pinfunction "MDI_TP_P1_38")
			(pintype "passive")
			(uuid "b37c6f48-a850-47aa-b3ec-6071a68d2774")
		)
		(pad "39" smd rect
			(at -9.3 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_TN_P1")
			(pinfunction "MDI_TN_P1_39")
			(pintype "passive")
			(uuid "e62d1db7-bad6-4804-92a5-017255896cf8")
		)
		(pad "40" smd rect
			(at -7.9 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_RP_P1")
			(pinfunction "MDI_RP_P1_40")
			(pintype "passive")
			(uuid "245508c5-cc7e-4729-b6af-4278ae82c547")
		)
		(pad "41" smd rect
			(at -6.5 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_RN_P1")
			(pinfunction "MDI_RN_P1_41")
			(pintype "passive")
			(uuid "b1a2549e-e1c4-4f30-a1ae-0a4e9810cdec")
		)
		(pad "42" smd rect
			(at -5.1 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_RP_P2")
			(pinfunction "MDI_RP_P2_42")
			(pintype "passive")
			(uuid "1828c68e-6faa-4bbb-bd39-2b620360cf56")
		)
		(pad "43" smd rect
			(at -3.7 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_RN_P2")
			(pinfunction "MDI_RN_P2_43")
			(pintype "passive")
			(uuid "926a6351-bf44-4e1d-a8e9-67ae662d3fe1")
		)
		(pad "44" smd rect
			(at -2.3 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_TP_P2")
			(pinfunction "MDI_TP_P2_44")
			(pintype "passive")
			(uuid "437680b1-6a03-4b29-aa3f-094dddc5947d")
		)
		(pad "45" smd rect
			(at -0.9 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "MDI_TN_P2")
			(pinfunction "MDI_TN_P2_45")
			(pintype "passive")
			(uuid "31fdbda0-ac51-42a4-8359-b7ad7ecd4c77")
		)
		(pad "46" smd rect
			(at 0.5 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-MDI_TP_P3-Pad46)")
			(pinfunction "MDI_TP_P3_46")
			(pintype "passive")
			(uuid "79fc4dc7-68e8-406f-90e7-b88239d2e1ad")
		)
		(pad "47" smd rect
			(at 1.9 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-MDI_TN_P3-Pad47)")
			(pinfunction "MDI_TN_P3_47")
			(pintype "passive")
			(uuid "9b903243-154b-494e-be1d-b7fadc6fe8e2")
		)
		(pad "48" smd rect
			(at 3.3 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-MDI_RP_P3-Pad48)")
			(pinfunction "MDI_RP_P3_48")
			(pintype "passive")
			(uuid "ca18ab88-b927-45a8-8497-27a174754272")
		)
		(pad "49" smd rect
			(at 4.7 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-MDI_RN_P3-Pad49)")
			(pinfunction "MDI_RN_P3_49")
			(pintype "passive")
			(uuid "97e70898-0d75-4a22-9515-5c89c0c54775")
		)
		(pad "50" smd rect
			(at 6.1 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-MDI_RP_P4-Pad50)")
			(pinfunction "MDI_RP_P4_50")
			(pintype "passive")
			(uuid "988c5aad-e9be-47d0-8891-19c54910f103")
		)
		(pad "51" smd rect
			(at 7.5 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-MDI_RN_P4-Pad51)")
			(pinfunction "MDI_RN_P4_51")
			(pintype "passive")
			(uuid "2806aa89-c208-46f0-8852-6f675433ba3f")
		)
		(pad "52" smd rect
			(at 8.9 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-MDI_TP_P4-Pad52)")
			(pinfunction "MDI_TP_P4_52")
			(pintype "passive")
			(uuid "896239da-e82c-4f1c-9a13-3e5819f46d2d")
		)
		(pad "53" smd rect
			(at 10.3 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-MDI_TN_P4-Pad53)")
			(pinfunction "MDI_TN_P4_53")
			(pintype "passive")
			(uuid "abdefbdc-a699-47d5-8377-f2601011765d")
		)
		(pad "54" smd rect
			(at 11.7 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-USB_DP-Pad54)")
			(pinfunction "USB_DP_54")
			(pintype "passive")
			(uuid "2aaa1516-deb3-493b-afa8-03c87b165235")
		)
		(pad "55" smd rect
			(at 13.1 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(IC1-USB_DM-Pad55)")
			(pinfunction "USB_DM_55")
			(pintype "passive")
			(uuid "e3059a24-86f6-4805-a70a-fac992465f97")
		)
		(pad "56" smd rect
			(at 14.5 9.35)
			(size 0.9 1.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_5_56")
			(pintype "passive")
			(uuid "5356b8fe-8685-4cea-9e50-9250f74195fd")
		)
		(pad "EP1" smd rect
			(at 11.65 2.55 90)
			(size 1.2 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "EP1_EP1")
			(pintype "passive")
			(uuid "ed496941-2550-4ed9-a9cf-3283f2c4668b")
		)
		(pad "EP2" smd rect
			(at 11.65 -4.05 90)
			(size 1.2 2.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "EP2_EP2")
			(pintype "passive")
			(uuid "504553de-b08f-452e-a3b2-cfbac107c0a9")
		)
		(pad "EP3" smd rect
			(at -3.6 0.25 90)
			(size 5 5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "EP3_EP3")
			(pintype "passive")
			(uuid "415b28ed-f6da-4eb5-9027-2bdba4b9cc06")
		)
		(embedded_fonts no)
		(model "HLK-7628N.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_RJ:RJ45_Hanrun_HR911105A_Horizontal"
		(layer "F.Cu")
		(uuid "dfe512b7-b8a5-4839-9a3f-e80f5fa36f2a")
		(at 85.135 33.565)
		(descr "1 Port RJ45 8P8C receptacle, shielded, with magnetics, through hole, 2 LEDs, tab down, http://www.hanrun.com/public/upload/down/2020/09-11/cc11be56d66bb63d5f1eeb85492439c0.pdf")
		(tags "RJ45 Magjack ethernet")
		(property "Reference" "J3"
			(at 4.44 -5 0)
			(layer "F.SilkS")
			(uuid "71242570-b51c-44df-893b-2b34a3ff82c0")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Value" "RJ45_Hanrun_HR911105A_Horizontal"
			(at 4.44 18.5 0)
			(layer "F.Fab")
			(uuid "04b6c8ae-c73f-4097-af86-c002e8e11bc2")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/1811141815_HANRUN-Zhongshan-HanRun-Elec-HR911105A_C12074.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "4fe14bf4-d71f-4539-aca9-d5f4fabb6acf")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property "Description" "1 Port RJ45 Magjack Connector Through Hole 10/100 Base-T, AutoMDIX"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
			(uuid "05bbc93e-711e-4c69-8023-2e4af7ca7fdc")
			(effects
				(font
					(size 1.27 1.27)
					(thickness 0.15)
				)
			)
		)
		(property ki_fp_filters "RJ45*Hanrun*HR911105A*")
		(path "/84fc85a3-800a-46f1-9919-113e90725f30")
		(sheetname "/Ethernet/")
		(units
			(unit
				(name "A")
				(pins "1" "4" "2" "3" "5" "6" "8" "SH" "7" "12" "11" "9" "10")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_line
			(start -3.92 -0.9)
			(end -3.92 0.9)
			(stroke
				(width 0.12)
				(type default)
			)
			(layer "F.SilkS")
			(uuid "d8f7f2a3-6232-4934-ad97-cb2d0607de49")
		)
		(fp_line
			(start -3.69 -4.15)
			(end -3.69 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "acd80ce9-30ff-46d1-9d6b-1a6a1ad9066b")
		)
		(fp_line
			(start -3.69 -4.15)
			(end 12.57 -4.15)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "94e1ceb8-0665-45ff-b926-7a959fa1c219")
		)
		(fp_line
			(start -3.69 4.93)
			(end -3.69 11.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "927689b2-0fb2-4645-817a-a894e4b171dc")
		)
		(fp_line
			(start 12.57 -4.15)
			(end 12.57 1.65)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "af24a589-c114-403c-b2e0-3c97516c9036")
		)
		(fp_line
			(start 12.57 4.93)
			(end 12.57 11.95)
			(stroke
				(width 0.12)
				(type solid)
			)
			(layer "F.SilkS")
			(uuid "2d2ff189-52bb-4e4f-aaec-f2f766b0b7a5")
		)
		(fp_line
			(start -5.06 2.57)
			(end -5.06 4.05)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "3520b7d1-8332-45f1-9933-08760e1390cc")
		)
		(fp_line
			(start -5.06 2.57)
			(end -4.08 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "d01847ee-48b1-4b52-a97d-695b47f72e7e")
		)
		(fp_line
			(start -5.06 4.05)
			(end -4.08 5.03)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "f46fec7d-7186-4eea-a02f-295ff49b782e")
		)
		(fp_line
			(start -4.08 -4.54)
			(end -4.08 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0b12d9a8-dd2c-43e3-a69c-0dfa0c8c1e50")
		)
		(fp_line
			(start -4.08 -4.54)
			(end 12.96 -4.54)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "7f318789-6f3e-400c-a3dd-c8ba20ee7d80")
		)
		(fp_line
			(start -4.08 5.03)
			(end -4.08 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "dab1a338-0164-431d-9e66-dbb5e6e1c63e")
		)
		(fp_line
			(start -4.08 17.76)
			(end 12.96 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "9ae8c541-7946-46ab-972e-759c0eadd4b8")
		)
		(fp_line
			(start 12.96 -4.54)
			(end 12.96 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "07067f21-6f08-4d14-829a-d1960d2cc07b")
		)
		(fp_line
			(start 12.96 5.03)
			(end 12.96 17.76)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "ee8ddd30-08e7-4d16-a778-425182529c3d")
		)
		(fp_line
			(start 13.94 2.57)
			(end 12.96 1.59)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "e503523f-3a56-4de0-8a24-26c890e439d3")
		)
		(fp_line
			(start 13.94 4.05)
			(end 12.96 5.03)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "15a1a7d1-0ec9-4a26-9344-b30142a67c11")
		)
		(fp_line
			(start 13.94 4.05)
			(end 13.94 2.57)
			(stroke
				(width 0.05)
				(type solid)
			)
			(layer "F.CrtYd")
			(uuid "0e6731b6-7cc5-4285-a96c-18e6cd72cced")
		)
		(fp_line
			(start -3.58 -4.04)
			(end -3.58 -1.01)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "3b4287e9-0b61-4785-9031-bcd557b08f47")
		)
		(fp_line
			(start -3.58 -4.04)
			(end 12.46 -4.04)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "c69b1d68-bee1-4521-96a2-af70dc8cbfb0")
		)
		(fp_line
			(start -3.58 0.99)
			(end -3.58 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "bb41860a-cbe0-473f-a0ca-819834f4b6f4")
		)
		(fp_line
			(start -3.58 17.26)
			(end 12.46 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "e8e89682-8a9e-45e4-a87d-4428a0490451")
		)
		(fp_line
			(start -2.58 -0.01)
			(end -3.58 -1.01)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "76ac0ab1-ad48-4687-b5fd-206d41a9d184")
		)
		(fp_line
			(start -2.58 -0.01)
			(end -3.58 0.99)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "48c56f99-0c0a-43db-a602-620fb51d6538")
		)
		(fp_line
			(start 12.46 -4.04)
			(end 12.46 17.26)
			(stroke
				(width 0.1)
				(type solid)
			)
			(layer "F.Fab")
			(uuid "074bdcc0-6d6c-4b19-a658-149f12864792")
		)
		(fp_text user "${REFERENCE}"
			(at 4.44 6.36 0)
			(layer "F.Fab")
			(uuid "73581107-e354-48a6-b7ba-9eb33748d50c")
			(effects
				(font
					(size 1 1)
					(thickness 0.15)
				)
			)
		)
		(pad "" np_thru_hole circle
			(at -1.275 6.36)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(uuid "bc03af29-21a4-40e9-8045-e5e366da60bf")
		)
		(pad "" np_thru_hole circle
			(at 10.155 6.36)
			(size 3.25 3.25)
			(drill 3.25)
			(layers "*.Cu" "*.Mask")
			(uuid "9b79199b-afe4-4d8f-a705-84f10399d993")
		)
		(pad "1" thru_hole roundrect
			(at 0 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.167)
			(net "MDI_TP_P1")
			(pinfunction "TD+_1")
			(pintype "passive")
			(uuid "75377614-cc88-477a-ba07-ad421d07467f")
		)
		(pad "2" thru_hole circle
			(at 1.26 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_TN_P1")
			(pinfunction "TD-_2")
			(pintype "passive")
			(uuid "6c645376-9f01-4d18-b9e9-391415f9d588")
		)
		(pad "3" thru_hole circle
			(at 2.54 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_RP_P1")
			(pinfunction "RD+_3")
			(pintype "passive")
			(uuid "7bae79ca-8f1a-4480-8c61-69fc80b03d4d")
		)
		(pad "4" thru_hole circle
			(at 3.8 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J3-TCT)")
			(pinfunction "TCT_4")
			(pintype "passive")
			(uuid "5ebefe99-677b-4500-abbc-8bf9ea9e5222")
		)
		(pad "5" thru_hole circle
			(at 5.08 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(J3-RCT)")
			(pinfunction "RCT_5")
			(pintype "passive")
			(uuid "8208a631-7f3e-448e-82ee-124a33d91250")
		)
		(pad "6" thru_hole circle
			(at 6.34 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "MDI_RN_P1")
			(pinfunction "RD-_6")
			(pintype "passive")
			(uuid "2f6ab3f4-db92-4b5d-ab6e-14a1db9a593e")
		)
		(pad "7" thru_hole circle
			(at 7.62 0)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J3-NC-Pad7)")
			(pinfunction "NC_7")
			(pintype "no_connect")
			(uuid "e3bf94ce-697f-4b25-aac0-0bc2b11c9da5")
		)
		(pad "8" thru_hole circle
			(at 8.88 -2.54)
			(size 1.5 1.5)
			(drill 0.89)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "power_in")
			(uuid "55df5afc-9340-4359-a68c-a9906e720a99")
		)
		(pad "9" thru_hole circle
			(at -2.185 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J3-Pad9)")
			(pintype "passive")
			(uuid "c42868a7-058f-4d60-909d-56b8d302587d")
		)
		(pad "10" thru_hole circle
			(at 0.355 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J3-Pad10)")
			(pintype "passive")
			(uuid "e37b48f4-787f-41fa-97fb-cfc9375941f9")
		)
		(pad "11" thru_hole circle
			(at 8.525 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J3-Pad11)")
			(pintype "passive")
			(uuid "b4e7b911-1b28-4ad3-92b7-2f9b0f31f40c")
		)
		(pad "12" thru_hole circle
			(at 11.065 11.26)
			(size 1.5 1.5)
			(drill 1.02)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(J3-Pad12)")
			(pintype "passive")
			(uuid "e177e047-c193-4d32-babe-5ecb170a67cd")
		)
		(pad "SH" thru_hole circle
			(at -3.305 3.31)
			(size 2.5 2.5)
			(drill 1.63)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
			(uuid "9c669680-8aec-4e8c-9da1-ab556208bcbe")
		)
		(pad "SH" thru_hole circle
			(at 12.185 3.31)
			(size 2.5 2.5)
			(drill 1.63)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pintype "passive")
			(uuid "1144c092-eade-4cd8-b6b6-61d3b2e591c3")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_RJ.3dshapes/RJ45_Hanrun_HR911105A_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(embedded_fonts no)
)
