
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "2171790001" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -12.7 16.002 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "2171790001" (id 1) (at -12.7 -18.542 0.0)
      (effects (font (size 1.27 1.27)) (justify top left))
    )
    (property "Footprint" "2171790001:MOLEX_2171790001" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MF" "Molex" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.16 mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Package" "None" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Price" "None" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Check_prices" "https://www.snapeda.com/parts/217179-0001/Molex/view-part/?ref=eda" (id 8) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 9) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "A1" (id 10) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "SnapEDA_Link" "https://www.snapeda.com/parts/217179-0001/Molex/view-part/?ref=snap" (id 11) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MP" "217179-0001" (id 12) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Description" "\n                        \n                            USB-C (USB TYPE-C) USB 2.0 Receptacle Connector 24 (16+8 Dummy) Position Surface Mount, Right Angle; Through Hole\n                        \n" (id 13) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "Availability" "In Stock" (id 14) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "Molex" (id 15) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "2171790001_0_0"
      (rectangle (start -12.7 -17.78) (end 12.7 15.24)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin power_in line (at 17.78 0.0 180.0) (length 5.08)
        (name "GND1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A1B12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -17.78 0.0 0) (length 5.08)
        (name "VBUS1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A4B9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 10.16 0) (length 5.08)
        (name "DP1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 12.7 0) (length 5.08)
        (name "CC1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 5.08 0) (length 5.08)
        (name "SBU1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 7.62 0) (length 5.08)
        (name "DN1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 17.78 -15.24 180.0) (length 5.08)
        (name "SHIELD4"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH4"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -2.54 180.0) (length 5.08)
        (name "GND2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B1A12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at -17.78 -2.54 0) (length 5.08)
        (name "VBUS2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B4A9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 7.62 180.0) (length 5.08)
        (name "DP2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 5.08 180.0) (length 5.08)
        (name "CC2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 12.7 180.0) (length 5.08)
        (name "SBU2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 10.16 180.0) (length 5.08)
        (name "DN2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 17.78 -7.62 180.0) (length 5.08)
        (name "SHIELD1"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 17.78 -10.16 180.0) (length 5.08)
        (name "SHIELD2"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin passive line (at 17.78 -12.7 180.0) (length 5.08)
        (name "SHIELD3"
          (effects (font (size 1.016 1.016)))
        )
        (number "SH3"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)